**Stormwater Management Program (SWMP)**

##MUNICIPALITY

**Permit Year 4**

EPA NPDES Permit Number NHR041000

# Certification

***Instructions: All reports, including SWPPPs, inspection reports, annual reports, monitoring reports, reports on training and other information required by this permit must be signed by a person described in Appendix B, Subsection 11.A or by a duly authorized representative of that person in accordance with Appendix B, Subsection 11.B. If there is an authorized representative to sign MS4 reports, there must be a signed and dated written authorization. Use the following language if your municipality wishes to file using an authorized representative.***

**Authorized Representative:**

The authorization letter is:

[ ]  Attached to this document (document name listed below):

[ ]  Publicly available at the website:

***Instructions: Use the following language if signed by a person described in Appendix B.***

“I certify under penalty of law that this document and all attachments were prepared under my direction or supervision in accordance with a system designed to assure that qualified personnel properly gathered and evaluated the information submitted. Based on my inquiry of the person or persons who manage the system, or those persons directly responsible for gathering the information, the information submitted is, to the best of my knowledge and belief, true, accurate, and complete. I am aware that there are significant penalties for submitting false information, including the possibility of fine and imprisonment for knowing violations.”

Printed Name

Signature Date

# Background

### Stormwater Regulation

The Stormwater Phase II Final Rule was promulgated in 1999 and was the next step after the 1987 Phase I Rule in EPA's effort to preserve, protect, and improve the Nation's water resources from polluted stormwater runoff. The Phase II program expands the Phase I program by requiring additional operators of MS4s in urbanized areas and operators of small construction sites, through the use of NPDES permits, to implement programs and practices to control polluted stormwater runoff. Phase II is intended to further reduce adverse impacts to water quality and aquatic habitat by instituting the use of controls on the unregulated sources of stormwater discharges that have the greatest likelihood of causing continued environmental degradation. Under the Phase II rule all MS4s with stormwater discharges from Census designated Urbanized Area are required to seek NPDES permit coverage for those stormwater discharges.

### Permit Program Background

On May 1, 2003, EPA Region 1 issued its Final General Permit for Stormwater Discharges from Small Municipal Separate Storm Sewer Systems (2003 small MS4 permit) consistent with the Phase II rule. The 2003 small MS4 permit covered "traditional" (i.e., cities and towns) and "non-traditional" (i.e., Federal and state agencies) MS4 Operators located in the states of Massachusetts and New Hampshire. This permit expired on May 1, 2008 but remained in effect until operators were authorized under the 2016 MS4 general permit, which became effective on July 1, 2018.

### Stormwater Management Program (SWMP)

The SWMP describes and details the activities and measures that will be implemented to meet the terms and conditions of the permit. The SWMP accurately describes the permittees plans and activities. The document should be updated and/or modified during the permit term as the permittee's activities are modified, changed or updated to meet permit conditions during the permit term. The main elements of the stormwater management program are (1) a public education program in order to affect public behavior causing stormwater pollution, (2) an opportunity for the public to participate and provide comments on the stormwater program (3) a program to effectively find and eliminate illicit discharges within the MS4 (4) a program to effectively control construction site stormwater discharges to the MS4 (5) a program to ensure that stormwater from development projects entering the MS4 is adequately controlled by the construction of stormwater controls, and (6) a good housekeeping program to ensure that stormwater pollution sources on municipal properties and from municipal operations are minimized.

**Town Specific MS4 Background** (optional)

# Small MS4 Authorization

The NOI was submitted on

The NOI can be found at the following (document name or web address):

[https://www.epa.gov/npdes-permits/regulated-ms4-new-hampshire-communities](http://www.epa.gov/npdes-permits/regulated-ms4-new-hampshire-communities)

Authorization to Discharge under the 2017 NH Small MS4 General Permit was granted on

<insert date authorization letter is received>

The Authorization Letter can be found (document name or web address):

# Stormwater Management Program Team

##### SWMP Team Coordinator:

Position/Title:

Name

Department

Phone Number

Email Address

##### SWMP Team:

Position/Title:

Name

Department

Phone Number

Email Address

Position/Title:

Name

Department

Phone Number

Email Address

Position/Title:

Name

Department

Phone Number

Email Address

Position/Title:

Name

Department

Phone Number

Email Address

**Receiving Waters**

The list of receiving waters, impairments and number of outfalls discharging to each waterbody segment has been included in the Notice of Intent. Impairments have been updated as described in the TMDLs and Water Quality Limited Waters section of this plan.

**Eligibility: Endangered Species and Historic Properties**

Endangered Species and Historic Properties eligibility information has been included in the Notice of Intent.

# MCM 1

## Public Education and Outreach

#### Permit Part 2.3.2

***Instructions: Use the following language if your municipality has no Nitrogen, Phosphorous or Bacteria Impairments.***

**Requirement Year 1**

**BMP: Septic System Maintenance*****required if more than 30% septic systems in MS4 area***

**Description:**

**Targeted Audience:** Septic System Owners

**Responsible Department/Parties:**

**Measurable Goal(s):**

**Message Date:** TBD

**Requirement Year 2**

**BMP: TBD**

**Description:** TBD

**Targeted Audience:** Developer/Construction

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**Requirement Year 3**

**BMP: TBD *may remove requirement if no industrial exists in MS4 area***

**Description:** TBD

**Targeted Audience:** Industrial

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**BMP: TBD**

**Description:** TBD

**Targeted Audience:** Businesses

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Spring

**Requirement Year 4**

**BMP: Septic System Maintenance*****required if more than 30% septic systems in MS4 area***

**Description:**

**Targeted Audience:** Septic System Owners

**Responsible Department/Parties:**

**Measurable Goal(s):**

**Message Date:** TBD

**BMP: TBD**

**Description:** TBD

**Targeted Audience:** Developer/Construction

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**Requirement Year 5**

**BMP: TBD *may remove requirement if no industrial exists in MS4 area***

**Description:** TBD

**Targeted Audience:** Industrial

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**BMP: TBD**

**Description:** TBD

**Targeted Audience:** Businesses

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Spring

***Instructions: Use the following language if your municipality has Bacteria Impairments but no Nitrogen or Phosphorous.***

**Requirement Year 1**

**BMP: Petwaste Disposal**

**Description:**

**Targeted Audience:** Pet Owners

**Responsible Department/Parties:**

**Measurable Goal(s):**

**Message Date:** Summer, time of license renewal, other

**BMP: Septic System Maintenance*****required once – may move to any year***

**Description:**

**Targeted Audience:** Septic System Owners

**Responsible Department/Parties:**

**Measurable Goal(s):**

**Message Date:** TBD

**Requirement Year 2**

**BMP: Petwaste Disposal**

**Description:** TBD

**Targeted Audience:** Pet Owners

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** TBD

**BMP: TBD**

**Description:** TBD

**Targeted Audience:** Developer/Construction

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**Requirement Year 3**

**BMP: Petwaste Disposal**

**Description:** TBD

**Targeted Audience:** Pet Owners

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** TBD

**BMP: TBD *may remove requirement if no industrial exists in MS4 area***

**Description:** TBD

**Targeted Audience:** Industrial

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**BMP: TBD**

**Description:** TBD

**Targeted Audience:** Businesses

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Spring

**Requirement Year 4**

**BMP: Petwaste Disposal**

**Description:** TBD

**Targeted Audience:** Pet Owners

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** TBD

**BMP: TBD**

**Description:** TBD

**Targeted Audience:** Developer/Construction

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**Requirement Year 5**

**BMP: Petwaste Disposal**

**Description:** TBD

**Targeted Audience:** Pet Owners

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** TBD

**BMP: TBD *may remove requirement if no industrial exists in MS4 area***

**Description:** TBD

**Targeted Audience:** Industrial

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**BMP: TBD**

**Description:** TBD

**Targeted Audience:** Businesses

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Spring

***Instructions: Use the following language if your municipality has Bacteria and Nitrogen or Phosphorous.***

**Requirement Year 1**

**BMP: Grass and Fertilizer**

**Description:** TBD

**Targeted Audience:** Residential &/or Business

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Spring

**BMP: Petwaste Disposal**

**Description:** TBD

**Targeted Audience:** Pet Owners

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Summer, time of license renewal, other

**BMP: Disposal of Leaf and Grass Clippings** ***remove this from year one if not done in fall***

**Description:** TBD

**Targeted Audience:** Residential &/or Business

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**BMP: Septic System Maintenance*****required once – may move to any year***

**Description:** TBD

**Targeted Audience:** Septic System Owners

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** TBD

**Requirement Year 2**

**BMP: Grass and Fertilizer**

**Description:** TBD

**Targeted Audience:** Residential &/or Business

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Spring

**BMP: Petwaste Disposal**

**Description:** TBD

**Targeted Audience:** Pet Owners

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** TBD

**BMP: Disposal of Leaf and Grass Clippings**

**Description:** TBD

**Targeted Audience:** Residential &/or Business

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**BMP: TBD**

**Description:** TBD

**Targeted Audience:** Developer/Construction

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**Requirement Year 3**

**BMP: Grass and Fertilizer**

**Description:** TBD

**Targeted Audience:** Residential &/or Business

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Spring

**BMP: Petwaste Disposal**

**Description:** TBD

**Targeted Audience:** Pet Owners

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** TBD

**BMP: Disposal of Leaf and Grass Clippings**

**Description:** TBD

**Targeted Audience:** Residential &/or Business

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**BMP: TBD may remove requirement if no industrial exists in MS4 area**

**Description:** TBD

**Targeted Audience:** Industrial

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**Requirement Year 4**

**BMP: Grass and Fertilizer**

**Description:** TBD

**Targeted Audience:** Residential &/or Business

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Spring

**BMP: Petwaste Disposal**

**Description:** TBD

**Targeted Audience:** Pet Owners

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** TBD

**BMP: Disposal of Leaf and Grass Clippings**

**Description:** TBD

**Targeted Audience:** Residential &/or Business

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**BMP: TBD**

**Description:** TBD

**Targeted Audience:** Developer/Construction

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**Requirement Year 5**

**BMP: Grass and Fertilizer**

**Description:** TBD

**Targeted Audience:** Residential &/or Business

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Spring

**BMP: Petwaste Disposal**

**Description:** TBD

**Targeted Audience:** Pet Owners

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** TBD

**BMP: Disposal of Leaf and Grass Clippings**

**Description:** TBD

**Targeted Audience:** Residential &/or Business

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**BMP: TBD *may remove requirement if no industrial exists in MS4 area***

**Description:** TBD

**Targeted Audience:** Industrial

**Responsible Department/Parties:**

**Measurable Goal(s):** TBD

**Message Date:** Fall

**MCM 2**

Public Involvement and Participation

Permit Part 2.3.3

**BMP: Public Review of Stormwater Management Program**

**Location of Plan and/or Web Address:**

**Responsible Department/Parties:**

**Measurable Goal(s):** Stormwater Management Plan is publicly available

**BMP: Public Participation in Stormwater Management Program Development**

**Description:**

**Responsible Department/Parties:**

**Measurable Goal(s):** Annual public input provided

**MCM 3**

Illicit Discharge Detection and Elimination (IDDE) Program

Permit Part 2.3.4

##### BMP: IDDE Legal Authority

See Illicit Discharge Detection and Elimination (IDDE) Plan

##### BMP: Sanitary Sewer Overflow (SSO) Inventory

See Illicit Discharge Detection and Elimination (IDDE) Plan

##### BMP: Map of Storm Sewer System

See Illicit Discharge Detection and Elimination (IDDE) Plan

**BMP: IDDE Program**

See Illicit Discharge Detection and Elimination (IDDE) Plan

**BMP: Employee Training**

See Illicit Discharge Detection and Elimination (IDDE) Plan

**MCM 4**

Construction Site Stormwater Runoff Control

Permit Part 2.3.5

##### BMP: Sediment and Erosion Control Ordinance

##### Completed (by May 1, 2008) [ ]

**Ordinances Link or Reference:**

**Department Responsible for Enforcement:**

##### BMP: Site Plan Review Procedures

##### Written procedures completed (by year 1) [ ]

**Document Name and/or Web Address:**

**Department Responsible for Enforcement:**

##### Description:

##### Measurable Goal(s): Conduct site plan review of 100% of projects according to the procedures outlined above.

##### BMP: Site Inspections and Enforcement of Sediment and Erosion Control Measures Procedures

##### Completed (by year 1) [ ]

**Document Name and/or Web Address:**

**Department Responsible for Enforcement:**

##### Description:

##### Measurable Goal(s): Inspect 100% of construction sites as outlined in the above document and take enforcement actions as needed.

**MCM 5**

Post Construction Stormwater Management in New Development and Redevelopment

Permit Part 2.3.6

##### BMP: Post-Construction Ordinance

##### Completed (by year 2) [ ]

**Town Ordinances Link or Reference:**

##### Department Responsible for Enforcement:

##### BMP: Street Design and Parking Lot Guidelines Report

##### Completed (by year 4) [ ]

**Document Name and/or Web Address:**

TBD

TBD

**Department Responsible for Enforcement:**

##### Description:

##### Measurable Goal(s): Recommendations are implemented by year 4 with progress reported annually.

##### BMP: Green Infrastructure Report

##### Completed (by year 4) [ ]

**Document Name and/or Web Address:**

TBD

**Department Responsible for Enforcement:**

TBD

##### Description:

##### Measurable Goal(s): Recommendations are implemented by year 4 with progress reported annually.

##### BMP: List of Municipal Retrofit Opportunities

##### Completed (by year 4) [ ]

**Document Name and/or Web Address:**

**Department Responsible for Enforcement:**

##### Description:

##### Measurable Goal(s): The list is completed by year 4 and updated as needed.

**MCM 6**

Good Housekeeping and Pollution Prevention for Permittee Owned Operations

Permit Part 2.3.7

**PERMITTEE OWNED FACILITIES**

##### BMP: Parks and Open Spaces Operations and Maintenance Procedures

##### Written Document Completed (by year 2) [ ]

**Document Name and/or Web Address:**

**Responsible Department/Parties:**

##### Description: Establish procedures to address the proper use, storage, and disposal of pesticides, herbicides, and fertilizers (PHF) including minimizing the use of these products in accordance with Section 2.3.7.1.a of the MS4 permit.

##### Measurable Goal(s): Implement the SOP on 100% of the parks and open spaces.

##### BMP: Buildings and Facilities Operations and Maintenance Procedures

##### Written Document Completed (by year 2) [ ]

**Document Name and/or Web Address:**

**Responsible Department/Parties:**

##### Description: Evaluate the use, storage, and disposal of petroleum products and other potential stormwater pollutants. Provide employee training as necessary, ensure that Spill Prevention Plans are in place. Develop management procedures for dumpsters and other waste management equipment. Sweep lots and areas surrounding the facilities clean to reduce runoff of pollutants in accordance with Section 2.3.7.1 b. of the MS4 permit.

##### Measurable Goal(s): Implement the SOP on 100% of buildings and facilities.

##### BMP: Vehicles and Equipment Operations and Maintenance Procedures

##### Written Document Completed (by year 2) [ ]

**Document Name and/or Web Address:**

**Responsible Department/Parties:**

##### Description: Establish procedures for the storage of permittee vehicles. Vehicles with fluid leaks shall be stored indoors of containment shall be provided. Evaluate fueling areas owned by the permittee or used by permitee vehicles. Establish procedures to ensure that vehicle wash waters are not discharged to municipal stormdrains or surface waters.

##### Measurable Goal(s): Implement the SOP on 100% of vehicles and equipment.

### INFRASTRUCTURE

**BMP: Catch Basin Cleaning Program**

##### Written Document Completed (by year 1) [ ]

**Document Name and/or Web Address:**

**Responsible Department/Parties:**

##### Description: The ##AGENCY OR DEPARTMENT performs routine inspections, cleaning, and maintenance of the approximately ##NUMBER OF CATCH BASINS catch basins that are located within the MS4 regulated area. The ##MUNICIPALITY will implement the following catch basin inspection and cleaning procedures to reduce the discharge of pollutants from the MS4.

##### Routine inspection and cleaning of catch basins. Catch basins should be cleaned such that they are no more than 50 percent full[[1]](#footnote-1) at any time. The ##MUNICIPALITY will initially inspect all catch basins within the regulated area within two (2) years of the effective date of the permit to evaluate sediment or debris accumulation and establish optimal inspection and maintenance frequencies to meet the “50 percent” goal.

* If a catch basin sump is more than 50 percent full during two consecutive routine inspections or cleaning events, the finding will be documented, the contributing drainage area will be investigated for sources of excessive sediment loading, and to the extent practicable, contributing sources will be addressed. If no contributing sources are found, the inspection and cleaning frequency will be increased.
* Catch basins located near construction activities (roadway construction, residential, commercial, or industrial development or redevelopment) will be inspected and cleaned more frequently if inspection and maintenance activities indicate excessive sediment or debris loadings (i.e., catch basins more than 50 percent full). Priority will also be given to catch basins that discharge to impaired waters.
* The following information will be included in each annual report:
	+ - * + Any action taken in response to excessive sediment or debris loadings
				+ Total number of catch basins
				+ Number of catch basins inspected
				+ Number of catch basins cleaned
				+ Total volume or mass of material removed from catch basins.

##### Measurable Goal(s): All catch basins are cleaned in accordance to the document above such that no catch basin is more than 50% full at any given time.

**BMP: Street Sweeping Program**

##### Written Document Completed (by year 1) [ ]

**Document Name and/or Web Address:**

**Responsible Department/Parties:**

##### Description: The ##MUNICIPALITY will implement the following street and parking lot sweeping procedures to reduce the discharge of pollutants from the MS4:

##### All streets with the exception of rural uncurbed roads with no catch basins or high-speed limited access highways will be swept and/or cleaned a minimum of once per year in the spring (following winter activities such as sanding).

##### More frequent sweeping will be considered for targeted areas based on pollutant load reduction potential, inspections, pollutant loads, catch basin cleaning or inspection results, land use, impaired waters, or other factors.

##### More frequent sweeping is required for municipally-owned streets and parking lots in areas that discharge to certain nutrient-impaired waters. Sweeping must be performed in these areas a minimum of two times per year, once in the spring (following winter activities such as sanding) and at least once in the fall (Sept 1 – Dec 1; following leaf fall)

##### For rural uncurbed roadways with no catch basins and limited access highways, the ##MUNICIPALITY will either meet the minimum frequencies above, or develop and implement an inspection, documentation, and targeted sweeping plan outlining reduced frequencies within two (2) year of the effective date of the permit and submit such plan with its year one annual report.

##### The following information will be included in each annual report:

##### Number of miles cleaned, or the volume or mass of material removed

**Measurable Goal(s):** Annually sweep 100% of all streets and municipal parking lots in accordance with the schedule listed above.

**BMP: Winter Road Maintenance Program**

##### Written Document Completed (by year 1) [ ]

**Document Name and/or Web Address:**

**Responsible Department/Parties:**

**Description:** The ##MUNICIPALITY will implement the following winter maintenance procedures to reduce the discharge of pollutants from the MS4:

##### Minimize the use and optimize the application of sodium chloride and other salt (while maintaining public safety) and consider opportunities for use of alternative materials.

##### Optimize sand and/or chemical application rates through the use, where practicable, of automated application equipment (e.g., zero velocity spreaders), anti-icing and pre-wetting techniques, implementation of pavement management systems, and alternate chemicals. Maintain records of the application of sand, anti-icing and/or de-icing chemicals to document the reduction of chemicals to meet established goals.

##### Prevent exposure of deicing product (salt, sand, or alternative products) storage piles to precipitation by enclosing or covering the storage piles. Implement good housekeeping, diversions, containment or other measures to minimize exposure resulting from adding to or removing materials from the pile. Store piles in such a manner as not to impact surface water resources, groundwater resources, recharge areas, and wells

##### Provide training for municipal employees on winter roadway maintenance procedures.

**Measurable Goal(s):** Evaluate at least one salt/chloride alternative for use in the municipality.

**BMP: Stormwater Treatment Structures Inspection and Maintenance Procedures**

##### Written Document Completed (by year 1) [ ]

**Document Name and/or Web Address:**

**Responsible Department/Parties:**

**Description:** Structural stormwater BMPs will be inspected annually at a minimum and maintained as needed.

**Measurable Goal(s):** Inspect and Maintain 100% of treatment structures to ensure property function.

**BMP: SWPPP**

##### Written Document Completed (by year 2) [ ]

**Document Name and/or Web Address:**

**Responsible Department/Parties:**

**Description:** Develop and implement a SWPPP for all municipally owned or operated facilities in accordance with Section 2.3.7.2 of the MS4 permit.

**Measurable Goal(s):** Develop and implement SWPPP’s for 100% of municipally owned facilities.

**Annual Evaluation**

**Year 1 Annual Report**

**Document Name and/or Web Address:**

**Year 2 Annual Report**

**Document Name and/or Web Address:**

**Year 3 Annual Report**

**Document Name and/or Web Address:**

**Year 4 Annual Report**

**Document Name and/or Web Address:** TBD

**Year 5 Annual Report**

**Document Name and/or Web Address:** TBD

**Year X Annual Report**

**Document Name and/or Web Address:** TBD

**TMDLs and Water Quality Limited Waters**

# Bacteria/Pathogens

**Per 2018 303d list the following waterbodies are water quality limited where Bacteria is the cause of impairment:**

|  |  |
| --- | --- |
| **Applicable Receiving Waterbody(ies)****as listed in applicable 303d lists** | **Name** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

**Per Appendix H the following water bodies are subject to a Bacteria TMDL. Please note that updated lists of waterbodies with TMDLs are not provided within this document. The permit states that, “Approved TMDLs” for discharges from the permittee’s MS4 are those that have been approved by EPA as of the issuance date of this permit.” (Section 2.2.1.a). TMDLs that had been approved at the time of the permits issuance will continue to follow the requirements outlined in Appendix F. Any waterbodies that received TMDLs after the issuance of the permit are required to meet the requirements outlined in Appendix H. These waterbodies have been identified in the note sections.:**

|  |  |
| --- | --- |
| **Applicable Receiving Waterbody(ies)****as listed in 2017 approved Appendix H** | **Name** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

Annual Requirements Beginning Year 1

Rank outfalls to these receiving waters as high priority for IDDE implementation in the initial outfall ranking (see IDDE Plan for ranking)

Annual message encouraging the proper management of pet waste, including noting any existing ordinances where appropriate as outlined in this SWMP

# Phosphorus Impairment

**Per Section 2.2.2 the ##Municipality is listed as having discharges within the watershed of impaired waterbodies or their tributaries due to phosphorus. Relative to total phosphorous (TP), the EPA MS4 permit created impairment lists based on both TP and TP-related impairments. The ##Municipality has not provided an update to this part of the analysis because the listing methodology employed by NHDES does not include TP-related impairments. The ##Municapality will continue to refer to the lists provided in the MS4 permit on pages 22 through 23.**

Annual Requirements Beginning Year 1

Rank outfalls to these receiving waters as high priority for IDDE implementation in the initial outfall ranking (see IDDE Plan for ranking).

Distribute an annual message that encourages the proper use and disposal of grass clippings and encourages the proper use of slow-release and phosphorus-free fertilizers as outlined in this SWMP.

Distribute an annual message encouraging the proper management of pet waste, including noting any existing ordinances where appropriate as outlined in this SWMP.

Distribute an annual message in the encouraging the proper disposal of leaf litter as outlined in this SWMP.

Increase street sweeping frequency of all municipal owned streets and parking lots subject to Permit part 2.3.7.a.iii.(c) to a minimum of two times per year (spring and fall) as outlined in this plan.

Establish procedures to properly manage grass cuttings and leaf litter on permittee property, including prohibiting blowing organic waste materials onto adjacent impervious surfaces.

Retrofit inventory and priority ranking under 2.3.6.1.b. shall include consideration of BMPs to reduce phosphorus discharges.

Any structural BMPs listed in Table 3 of Attachment 1 to Appendix H already existing or installed in the regulated area by the permittee or its agents shall be tracked and the permittee shall estimate the phosphorus removal by the BMP consistent with Attachment 1 to Appendix H. Document the BMP type, total area treated by the BMP, the design storage volume of the BMP and the estimated phosphorus removed in pass per year by the BMP in each annual report.

Requirements Due by Year 2

The requirement for adoption/amendment of the permittee's ordinance or other regulatory mechanism shall include a requirement that new development and redevelopment stormwater management BMPs be optimized for phosphorus removal.

Requirements Due by Year 4

Complete a Phosphorus Source Identification Report.

The document name (if attached) and/or web address is/are: TBD

Retrofit inventory and priority ranking under 2.3.6.1.b. shall include consideration of BMPs that infiltrate stormwater where feasible.

Requirements Due by Year 5

Evaluate all permittee-owned properties identified as presenting retrofit opportunities or areas for structural BMP installation under Permit part 2.3.6.d.ii or identified in the Phosphorus Source Identification Report that are within the drainage area of the impaired water or its tributaries.

Complete a listing of planned structural BMPs and a plan and schedule for implementation.

# Nitrogen Impairment

**Per Section 2.2.2 the ##MUNICIPALITY is listed as having discharges within the watershed of impaired waterbodies or their tributaries due to nitrogen. Because the entire MS4 area is within this watershed, the applicable BMP’s are being implemented throughout the entire watershed and not only focused on individual receiving waterbodies listed in the 303d list.** **Please note that there have been no changes to the list of waterbodies having total nitrogen impairments or draining to total nitrogen impaired waters supplied by EPA in the MS4 permit.**

Annual Requirements Beginning Year 1

Rank outfalls to these receiving waters as high priority for IDDE implementation in the initial outfall ranking (See IDDE Plan for ranking).

Distribute an annual message that encourages the proper use and disposal of grass clippings and encourages the proper use of slow-release fertilizers as outlined in this SWMP.

Distribute an annual message encouraging the proper management of pet waste, including noting any existing ordinances where appropriate as outlined in this SWMP.

Distribute an annual message encouraging the proper disposal of leaf litter as outlined in this SWMP.

Establish requirements for the use of slow release fertilizers on permittee owned property currently using fertilizer, in addition to reducing and managing fertilizer use as provided in part 2.3.7.1.

Establish procedures to properly manage grass cuttings and leaf litter on permittee property, including prohibiting blowing organic waste materials onto adjacent impervious surfaces.

Increase street sweeping frequency of all municipal owned streets and parking lots subject to Permit part 2.3.7.a.iii.(c) to a minimum of two times per year (spring and fall) as included in this SWMP.

Any structural BMPs listed in Table 3 of Attachment 1 to Appendix H already existing or installed in the regulated area by the permittee or its agents shall be tracked and the permittee shall estimate the nitrogen removal by the BMP consistent with Attachment 1 to Appendix H.

Requirements Due by Year 2

The requirement for adoption/amendment of the permittee's ordinance or other regulatory mechanism shall include a requirement that new development and redevelopment stormwater management BMPs be optimized for nitrogen removal.

Requirements Due by Year 4

Complete a Nitrogen Source Identification Report.

The document name (if attached) and/or web address is/are: TBD

Retrofit inventory and priority ranking under 2.3.6.1.b. shall include consideration of BMPs to reduce nitrogen discharges.

Requirements Due by Year 5

Evaluate all permittee-owned properties identified as presenting retrofit opportunities or areas for structural BMP installation under Permit part 2.3.6.d.ii or identified in the Nitrogen Source Identification Report that are within the drainage area of the impaired water or its tributaries.

Complete a listing of planned structural BMPs and a plan and schedule for implementation.

# Solids, Oil and Grease (Hydrocarbons), or Metals Impairments

**Per 2018 303d list the following waterbodies are water quality limited where Solids, Oil and Grease, or Metals are the cause of impairment:**

|  |  |
| --- | --- |
| **Applicable Receiving Waterbody(ies)** | **TMDL/Impairment Name**(if applicable) |
|  |  |
|  |  |
|  |  |

Annual Requirements Beginning Year 1

Rank outfalls to these receiving waters as high priority for IDDE implementation in the initial outfall ranking (See IDDE Plan for ranking).

Increase street sweeping frequency of all municipal owned streets and parking lots to a schedule to target areas with potential for high pollutant loads as prescribed by this SWMP.

Prioritize inspection and maintenance for catch basins to ensure that no sump shall be more than 50 percent full; Clean catch basins more frequently if inspection and maintenance activities indicate excessive sediment or debris loadings as prescribed by this SWMP.

Requirements Due by Year 2

Stormwater management systems designed on commercial and industrial land use area draining to the water quality limited water body shall incorporate designs that allow for shutdown and containment where appropriate to isolate the system in the event of an emergency spill or other unexpected event.

# Lake and Pond Phosphorus TMDL

**Per Appendix H the following water bodies are subject to a Lake and Pond Phosphorus TMDL. Please note that updated lists of waterbodies with TMDLs are not provided within this document. The permit states that, “Approved TMDLs” for discharges from the permittee’s MS4 are those that have been approved by EPA as of the issuance date of this permit.” (Section 2.2.1.a). TMDLs that had been approved at the time of the permits issuance will continue to follow the requirements outlined in Appendix F. Any waterbodies that received TMDLs after the issuance of the permit are required to meet the requirements outlined in Appendix H. These waterbodies have been identified in the note sections.:**

|  |  |  |
| --- | --- | --- |
| **Applicable Receiving Waterbody(ies)** | **PCP Complete** | **TMDL/Impairment Name**(if applicable) |
|  |[ ]   |
|  |[ ]   |
|  |[ ]   |

# Chloride Impairment

**Per 2018 303d list the following waterbodies are water quality limited where Chloride is the cause of impairment:**

|  |  |
| --- | --- |
| **Applicable Receiving Waterbody(ies)** | **TMDL/Impairment Name**(if applicable) |
|  |  |
|  |  |
|  |  |

Annual Requirements Beginning Year 1

Rank outfalls to these receiving waters as high priority for IDDE implementation in the initial outfall ranking (See IDDE Plan for ranking).

Requirements Due by Year 3

Develop a Salt Reduction Plan.

Requirements Due by Year 4

Continue implementation of the Salt Reduction Plan.

Requirements Due by Year 5

Fully implement the Salt Reduction Plan.

**Per Appendix H the following water bodies are subject to a Chloride TMDL. Please note that updated lists of waterbodies with TMDLs are not provided within this document. The permit states that, “Approved TMDLs” for discharges from the permittee’s MS4 are those that have been approved by EPA as of the issuance date of this permit.” (Section 2.2.1.a). TMDLs that had been approved at the time of the permits issuance will continue to follow the requirements outlined in Appendix F. Any waterbodies that received TMDLs after the issuance of the permit are required to meet the requirements outlined in Appendix H. These waterbodies have been identified in the note sections.:**

|  |  |
| --- | --- |
| **Applicable Receiving Waterbody(ies)****as listed in 2017 approved Appendix H** | **Name** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

Annual Requirements Beginning Year 1

Develop and implement a Chloride Reduction Plan.

1. [↑](#footnote-ref-1)